Insulation Displacement Connectors

The IDCs require testing before any start of validation so all designs are theoretical.

The only design changes made were to put a V-shaped taper on the cutting sides so that there is a more gradual cutting process than vertical cutting sides.

For more information on the IDCs, see the final reports in “\9. Deliverables”.